1. No comments from us, please proceed as you prefer.
2. All suggested components are acceptable
3. All suggested components are acceptable
4. Please use the following
   1. C43, C44: please use a generic 0603 1.5 uF capacitor, such as 06036D155KAT2A
   2. IC8: Use DS90LV028AQMA/NOPB
   3. J4: Use the part from TE Connectivity, 1888247‐1
   4. C30, C34: use MC0402B102K160CT. 16 V is fine.
5. Please use parts suggested in point 2)
6. Please use parts defined in PCBA Visualizer
7. For IC4 please use either Si5394A-A-GM. Available from Digikey 336-4800-ND
8. QZ1: please disregard information on BOM and use DSC1103CI5-050.0000 (3.2x2.5 package). Available from Mouser 998-1103CI5-050.0000
9. See point 8)
10. Please see following:
    1. J7: can also use ASP-134606-01. For instance Mouser 200-ASP-134606-01 or Digikey SAM8733-ND
    2. R47, R48, R49: use a generic 0603 resistor, 33 ohm, 1%, such as CRGP0603F33R
    3. REG1: use TPS799185DDCR, available from Mouser 595-TPS799185DDCR
11. All suggested components are acceptable
12. Ignore polarization marking